**Description**

|  |  |  |
| --- | --- | --- |
| *Luminaire Type* | : | **LED Steplight Recessed (entrance)** |
| *Luminaire Reference*  **ST-1X** | : | **MAERICH Popeye 1/2 TURBO 02-02 or equal** |
| *Lamp* | : | **LED warm white 2700K/2Watt/700mA/ASYMMETRIC** |
| *Lamp Reference* | : | **Cree LED comes with fixture manufacture** |
| *Gears* | : | **Remote DIMMBALE Driver inside IP Box 67 (by manufacture)** |
| *Accessories* | : | **Niche S1,**  **IP68 Connector 600mm spare Cable length** |

**  **

****

**Dimension**

|  |  |  |
| --- | --- | --- |
| *Recessed niche* | : | **120 mm** |
| *Opening niche* | : | **45 mm** |
| *Diameter* | : | **52 mm** |
| *Height top* | : | **13.5 mm** |
| *Weight* | : | **0.5 Kg** |

**Technical Specification**

|  |  |  |
| --- | --- | --- |
| *Reflector* | : | Lamp reflector |
| *Housing* | : | Black aluminium body  Anti glare with frosted safety glass cover  INTELLIMODE |
| *Cover Trim* | : | **Black Finish** |
| *Approval* | : | **IP 67** |
| *Transformer* | : | **Remote driver inside IP BOX 67 (by manufacture)**  **Trafo location should be coordinated on site** |

**PHOTOMETRIC DATA OF**

****

** **

****