**Description**

|  |  |  |
| --- | --- | --- |
| Luminaire Type | : | **LED Linear Uplighter surface (façade guest room 2)** |
| Luminaire Reference | : | **Maerich AQUA BATON 3S -03 or equal** |
| Lamp | : | **LED warmwhite 2700K/700mA/ ± 16Watt/16deg** |
| Lamp Reference | : | **Cree LED comes with fixture manufacture** |
| Gears | : | **Remote DIMMABLE DRIVER inside IP BOX IP67 (by manufacture)** |
| Accessories | : | **1 pair of adjustable mounting brackets ,  3000mm spare cable (include manufacture)**  **IP 68 Connector**  **MINILOUVRE + LINEAR HOOD** |

****

**UW-UP1**

****

**Dimension**

|  |  |  |
| --- | --- | --- |
| Height | : | **70 mm** |
| Width | : | **50 mm** |
| Length | : | **346 MM** |
| weight | : | **1.6 kg** |

**Technical Specification**

|  |  |  |
| --- | --- | --- |
| *Reflector* | : | Lamps LED |
| *Housing* | : | Electro polished stainless steel 316L  **with clear glass cover**  **UV resistant PMMA Cover**  **Included clip and Adjustable bracket** |
|  |  | **INTELLIMODE** |
| *Lamp Holder* | : | By manufacture |
| *Light Distribution* | : | **Medium distribution, 16deg** |
| *Approval* | : | IP 68 |
| *Transformer* | : | **Remote DIMMABLE INSIDE IP BOX IP 67 (by manufacture)**  **location should be coordinated on site** |

****