**Description**

|  |  |  |
| --- | --- | --- |
| *Luminaire Type* | : | **LED Uplighter floor Recessed (architrave windows)** |
| *Luminaire Reference* | : | **Maerich Popcorn 2 Turbo Recessed 02-01or equal** |
| *Lamp* | : | **LED warm white 2700K/2Watt/700Ma/10deg** |
| *Lamp Reference* | : | **Cree LED comes with fixture manufacture** |
| *Gears*  **UP-L1** | : | **Remote Dimmable Driver inside IP Box 67**  **(by manufacture) With cable control 1-10V** |
| *Accessories* | : | **DEEP WITH BLACKOUT RING- 02 Black aluminium finish**  **Clear Glass, Niche S1**  **IP 68 Connector,  600mm Neoprene Cable.** |

 

** **



**Dimension**

|  |  |  |
| --- | --- | --- |
| *Diameter* | : | **48 mm** |
| *Opening* | : | **46 mm** |
| *Recessed Depth* | : | **80 mm** |
| *Depth + Housing* |  | **120 mm** |
| *Cover height* | : | **2mm** |
| *Weight* | : | **0.3 kg** |

**Technical Specification**

|  |  |  |
| --- | --- | --- |
| *Reflector* | : | Lamp reflector |
| *Housing* | : | Black aluminium body  with clear safety glass cover  **INTELLIMODE** |
| *Cover trim* | : | **Anodised aluminium finish** |
| *Lamp Holder* | : | By manufacture |
| *Light Distribution* | : | **Spot 10° Light Distribution** |
| *Approval* | : | IP 67 |
| *Transformer* | : | **Remote Dimmable driver Inside IP BOX 67(by manufacture)**  **Trafo location should be coordinated on site** |

  