**Description**

|  |  |  |
| --- | --- | --- |
| *Luminaire Type* | : | **LED Adjustable Spotlight (danau)** |
| *Luminaire Reference* | : | **BRONZELITE SPOTLIGHT TL6000 or equal**  **FL-1X**  **(REVISI)** |
| *Lamp* | : | **LED Halogen PAR30/E27/20watt/2700K/15deg** |
| *Lamp Reference* | : | **LED comes with fixture manufacture** |
| *Gears* | : | **NON DIM Integrated Driver (by manufacture)** |
| *Accessories* | : | **Glare shield**  **Surface mount base & IP 68 Connector** |

** **

**Dimension**

|  |  |  |
| --- | --- | --- |
| *Diameter* | : | **1.40 mm** |
| *Height* | : | **241mm** |
| *width* | : | **- mm** |
| *Weight* | : | **2.5 kg** |

**Technical Specification**

|  |  |  |
| --- | --- | --- |
| *Housing* | : | **Die cast aluminium alloy, BLACK finish**  **With safety galss** |
| *Light Distribution* | : | **Wide beam 15deg** |
| *Adjustment* | : | Adjustable rotated |
| *IP* | : | IP 67 |
| *Transformer* | : | **Integrated Driver (by manufacture)**  **Trafo location should be coordinated on site.** |

