**Description**

|  |  |  |
| --- | --- | --- |
| *Luminaire Type* | : | **LED light Linear INSIDE Perimeter BARISOL/MEMBRAN (car display)** |
| *Luminaire Reference* | : | **ARCO SLIM LED LINE (IP 20) length 1mtr or equal** |
| *Lamp* | : | **LED WARM WHITE 3000K/24VDC/12Watt/Strip/meter**  **SL-BR2** |
| *Lamp Reference* | : | **By manufacture** |
| *Gears* | : | **DALI DIMMABLE Driver (by manufacture)** |
| *Accessories* | : | **With acrylic cover**  **Mounting clips for rail & IP 20 Connector & End cap** |



**Dimension**

|  |  |  |
| --- | --- | --- |
| *Width* | : | **20 mm** |
| *Length* | : | **1000 mm** |
| *Height* | : | **25 mm** |
| *Weight* | : | **0.25 Kg** |

** **

**Technical Specification**

|  |  |  |
| --- | --- | --- |
| *Housing* | : | **Extruded aluminium, black finish**  **With Frosted glass** |
| *Lamp Holder* | : | **By manufacture** |
| *Light Distribution* | : | **Diffuse distribution, 120 degree** |
| *Approval* | : | **IP 20** |
| *Transformer* | : | **Remote DALI DIMMABALE (by manufacture)**  **Trafo location should be coordinated** |
|  |  |  |